***IR Speaker Camera Instructions***

***Can pair with any Poker Analyzer***

Instructions

Congratulations on the purchase of one of the most discrete Poker Analyzer External cameras on the market. The Long Range Speaker camera is a great choice for playing games with one dealer, since the long range speaker box can lurk in the background.

Your package contains:

* Speaker Box containing: subwoofer, 2 speakers, remote, and the Aux cord

Here are the step by step instructions:

1. Set everything up. Find a place to mount the speaker box (roughly around 8 feet 8 inches).
2. Connect the speakers with the subwoofer. The camera is located in the subwoofer box receiver.
3. Open the game choice you are playing and find Video Settings. Change the settings from Local Camera to Wireless 2.57g. Go into the game like you are going to play.
4. At first the screen will be static looking all white. Use the remote control to connect the analyzer with the speaker box.
5. Practice, Practice, Practice! See how far or close you can go with a positive read on the cards. Make sure you know your limits so when you really play. The remote can turn the camera left/right/up/down. The light on the far camera will show where it is zoomed in on. When you change camera’s you will zoom in and read the cards.

Additional accessories:

We are offering Thumpers to Poker Analyzer customers. This is a remote that you click a button and it vibrates a player. Great for Dealer to player communications! Designed for the Poker Analyzer Dealer players who signal their friend/teammate.

For online video instructions visit: [www.howtomarkcards.com/speaker-Setup.html](http://www.howtomarkcards.com/speaker-Setup.html) (there is a step by step video instruction to help you set up your Speaker system!)